For 1990-2009 cars

### Removal Procedure

1. Remove the front side door trim. Refer to Front Side Door Trim Panel Replacement .
2. Starting at the top, pull downward on the front side door water deflector (3) in order to remove from the door edges (4).
3. Unroute any electrical connectors (2) and the front side door inside handle rod (1) from the water deflector (3), while removing the deflector from the vehicle.

### Installation Procedure

1. Route the electrical connectors (2) and the front side door inside handle rod (1) through the front side door water deflector (3).
2. Install the front side door water deflector (3) to the door (4).
3. Install the front side door trim. Refer to Front Side Door Trim Panel Replacement .