For 1990-2009 cars

#### Tools Required

• | J 26941 Pinion Shaft and Countergear Bearing Cup Remover

• | J 23907 Slide Hammer

• | J 35553 Differential Side Bearing Seal Installer

• | J 36850 Transmission Assembly Lubricant

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the 6 bolts and the left splash shield (1) from the vehicle.
3. Remove the front tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
4. Remove the drive axle from the vehicle. Refer to Wheel Drive Shaft Replacement in Wheel Drive Shafts.
5. Remove the drive axle shaft fluid seal (1) from the transaxle using J 26941 with J 23907 .
6. Inspect the differential-side joint surface of the drive axle assembly where the drive axle makes contact with the drive axle shaft fluid seal.

The surface should be smooth and free of any burrs or scarring which may damage the drive axle shaft fluid seal.

If damage to the differential-side joint is evident, replace the differential-side joint.

### Installation Procedure

1. Install the new drive axle shaft fluid seal (1) into the transaxle using the following tools:

• | For the driver's side, use J 35553 and a hammer.

• | For the passenger's side, use a hammer and a socket.

2. Apply J 36850 to the new drive axle shaft fluid seal lip.
3. Install the drive axle into the vehicle. Refer to Wheel Drive Shaft Replacement in Wheel Drive Shafts.
4. Install the front tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the left splash shield (1) to the vehicle. Secure the splash shield with the 6 bolts.

Tighten
Tighten the left splash shield bolts to 5 N·m (44 lb in).

6. Lower the vehicle.
7. Refill the transaxle, as necessary. Refer to Transmission Fluid Check .