For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment lid.
2. Remove the rear compartment lid lock cylinder rod (6) from the rear compartment lid lock cylinder (5).
3. Remove the following items from the rear compartment lid:

• | The retaining clip (4)

• | The rear compartment lid lock cylinder (5)

### Installation Procedure

1. Install the rear compartment lid lock cylinder (5) to the rear compartment lid. Secure the lock cylinder with the retaining clip (4).
2. Install the rear compartment lid lock cylinder rod (6) to the rear compartment lid lock cylinder (5).
3. Close the rear compartment lid.