For 1990-2009 cars

Important: Perform this procedure in order to prevent deployment of the air bags from the reserve energy supply power.

1. Remove the CIG and IGN Fuses from the junction block (1), which is located near the base of the steering column.
2. Remove the lower steering column trim cover.
3. Turn the steering wheel so that the vehicle's wheels are pointing straight ahead.
4. Remove the key from the ignition switch.
5. Release the inflatable restraint steering wheel module coil connector locking mechanism.
6. Disconnect the inflatable restraint steering wheel module coil connector C3 (1).
7. Remove the IP compartment (2). Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.
8. Release then unlock the IP module connector (1).
9. Disconnect the IP module pigtail.
10. Release and unlock the driver and passenger seat module connectors (1).
11. Disconnect the driver and passenger seat modules.