For 1990-2009 cars

#### Tools Required

• | J 44707 T Bar Push Puller

• | J 44736 Bridge and Forcing Screw

• | J 44737 Shift Rail Bearing Remover

• | J 44738 Bearing Remover

1. Remove the back-up lamp switch.
2. Remove the reverse gear idler shaft bracket bolt with the O-ring seal.
3. Remove and discard the O-ring seal.
4. Remove the reverse gear idler shaft bracket. Rotate the bracket to aid in removal.
5. Remove the reverse gear idler shaft.
6. Remove the reverse idler gear bearings.
7. Remove the reverse idler gear.
8. If RWD, remove the mainshaft rear oil seal and discard.
9. If 4WD, remove the mainshaft rear bearing O-ring seal and discard.

Important: Only remove the bearings if replacing the bearings. Do not use the bearings again after removal.

10. Inspect the bearings for damage or wear. Refer to Bearings and Spacers Cleaning and Inspection .
11. Remove the rear case shift rail bearing using the J 44707 (1) and the J 44737 (2). Expand the J 44737 to fit securely in the bearing.

Important: Only remove the bearings if replacing the bearings. Do not use the bearings again after removal.

12. Inspect the bearings for damage or wear. Refer to Bearings and Spacers Cleaning and Inspection .
13. Remove the countershaft rear bearing from the rear case using the J 44736 (1) and the J 44738 (2). Expand the J 44738 to fit securely in the bearing.