For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door inside handle. Refer to Rear Side Door Inside Handle Replacement .
2. Unclip and remove the trim cover (2) from the rear side door trim panel (1).
3. Remove the 2 screws (3) that retain the door trim panel (2).
4. Remove the rear side door window regulator handle by using a cloth to pull off the snap ring, if equipped.
5. Using a taped flat bladed tool, gently pry the rear side door window switch bezel (2) from the rear side door trim (1), if equipped.
6. Disconnect the rear side door window switch electrical connector (2), if equipped.
7. Remove the rear side door window switch bezel (3) from the vehicle, if equipped.
8. Remove the 2 plastic retainers (1, 5) that retain the rear side door trim (2).
9. Unclip and remove the rear side door trim (2) from the door by disengaging the plastic retainers.

### Installation Procedure

1. Position and install the rear side door trim (2) to the door and press the plastic retainers into place. Ensure that the plastic retainers are completely engaged. Secure the door trim with the 2 plastic retainers (1, 5).
2. Connect the rear side door window switch electrical connector (2), if equipped.
3. Install the rear side door window switch bezel (3) to the rear side door trim (1), if equipped.
4. Install the rear side door window regulator handle snap ring (1) to the rear side door window regulator handle (2), if equipped.
5. Install the regulator handle (2) to the door, if equipped.
6. Install the 2 screws (3) that retain the rear door trim panel (2).
7. Install the trim cover to the rear side door armrest.
8. Install the rear side door inside handle. Refer to Rear Side Door Inside Handle Replacement .