For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel assembly. Refer to Instrument Panel Assembly Replacement .
2. Remove the following components from the instrument panel (2):

• | The 1 screw

• | The right I/P outer air outlet

• | The plastic retainer

• | The left I/P outer air outlet

• | The 2 screws

• | The 6 wire harness retainers

• | The instrument panel wiring harness (5)

### Installation Procedure

1. Install the instrument panel wiring harness (5) to the instrument panel assembly (2). Secure the harness with the following:

• | The 6 wire harness retainers

• | The 2 screws

2. Install the left I/P outer air outlet to the instrument panel assembly. Secure the duct with the plastic retainer.
3. Install the right I/P outer air outlet to the instrument panel assembly. Secure the duct with the screw.
4. Install the instrument panel assembly. Refer to Instrument Panel Assembly Replacement .