For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 22912-01 Bearing Puller

• | J 35378 Bearing Puller Pilot

Use J 22912-01 and J 35378 in order to remove the intermediate shaft rear bearing

### Installation Procedure

#### Tools Required

J 35565 Intermediate Shaft Bearing Installer

1. UseJ 35565 in order to install the intermediate shaft rear bearing.
2. Verify that the distance from the gear flange end to the intermediate shaft is approximately 115.8 mm (4.559 inch).