For 1990-2009 cars

1. Remove the TV cable retaining bolt from the TV cable (1).
2. Remove the solenoid wire harness retaining bolt from the solenoid wire harness (2).
3. Remove the following components from the transaxle case (1):

• | 18 bolts

• | The transaxle fluid pan (2)

• | The gasket

4. Remove the following from the valve body assembly (1):

• | Three bolts

• | The fluid filter screen (2)

• | The gasket

5. Remove the electrical connectors (1) from the following components:

• | Shift solenoid No. 1 (3)

• | Shift solenoid No. 2 (2)

• | The torque converter clutch (TCC) solenoid

6. Remove one bolt and the solenoid wire harness clip (2) from the valve body assembly.
7. Remove the solenoid wire harness (1) from the transaxle case (2).
8. Disconnect the TV cable (1) from the throttle valve cam (2).
9. Remove the TV cable (1) from the transaxle case (2).
10. Remove 22 bolts (1) and the valve body assembly (2) from the transaxle case (while disconnecting the manual valve link).
11. Remove one bolt and the manual detent spring (1) from the transaxle case (2).
12. Disconnect the manual valve link (2) from the manual detent lever.
13. Remove the check ball body (1) and spring (3) from the transaxle case (2).
14. Remove the intermediate brake apply seal (1) from the transaxle case.
15. Remove the intermediate brake apply tube (1) from the transaxle case.

Important: When using compressed air to remove components, air pressure should not exceed 98 kPa (14 psi).

16. Remove the B2 accumulator piston (1) and spring from the transaxle case by slowly applying low pressure compressed air into the fluid passage (2).
17. Remove the two seals from the B2 accumulator piston.
18. Remove the C2 accumulator piston (1) and spring from the transaxle case by slowly applying low pressure compressed air into the fluid passage (2).
19. Remove the two seals from the C2 accumulator piston.
20. Remove the C1 accumulator piston (1) and spring from the transaxle case by slowly applying low pressure compressed air into the fluid passage (2).
21. Remove the one seal from the C1 accumulator piston.
22. Remove the C3 accumulator piston (1) and the spring from the transaxle case by slowly applying low pressure compressed air into the fluid passage (2).
23. Remove two seals from the C3 accumulator piston.
24. Remove the following components from the transaxle case:

• | One bolt

• | The second coast brake band guide (1)

25. Use a hammer and chisel in order to remove the manual lever hub protection sleeve (1) from the manual detent lever hub.

Important: Do NOT drop the roll pin into the transaxle case.

26. Use a standard drift punch and hammer in order to remove one roll pin from the manual detent lever hub (1).
27. Remove the retaining spring (2) from the manual shaft (1).
28. Remove the following components from the transaxle case:

• | The manual shaft (2)

• | The manual detent lever (1) and washer

29. Remove the manual shaft fluid seal (2) from the transaxle case (1).