For 1990-2009 cars

#### Tools Required

• | J 7872 Magnetic Base Indicator Set

• | J 23327 Clutch Spring Compressor

• | J 37282 Underdrive Brake Piston Compressor

1. Use the J 7872 in order to measure the underdrive brake assembly (1) clearance.
2. Apply 392-785 kPa (57-114 psi) of compressed air into the underdrive brake apply passage (2). Measure the underdrive brake assembly clearance.
3. The underdrive brake assembly clearance should fall within 1.070-2.050 mm (0.0421-0.0807 in).
4. If the underdrive brake assembly clearance does not fall within specification, inspect the underdrive brake assembly components for excessive wear or damage.
5. Install a J 23327 with a J 37282 and compress the underdrive brake piston return spring until the underdrive brake piston return spring snap ring (1) can be removed.
6. Remove the underdrive brake piston return spring snap ring (1) from the transaxle case.
7. Remove the J 23327 and the J 37282 from the transaxle case.
8. Remove the underdrive brake flange (2), the three plates (1) and the three discs (3) from the transaxle case.
9. Remove the underdrive brake piston return spring (2) from the transaxle case (1).
10. Remove the two seal rings (1) from the underdrive clutch drum support (2).

Caution: Wear safety glasses in order to avoid eye damage.

Notice: When using compressed air to remove components, air pressure should not exceed 98 kPa (14 psi).

11. Remove the underdrive brake piston from the transaxle case by slowly applying low pressure compressed air into the underdrive brake apply passage (2).