For 1990-2009 cars

### Removal Procedure

1. Lower the window.
2. Remove the front side door trim. Refer to Front Side Door Trim Panel Replacement .
3. Remove the water deflector (3) from the front door (4).
4. Unclip and remove the inner mirror garnish (2) from the door.
5. Remove the window run channel weatherstrip (2) from the guide channel.

### Installation Procedure

1. Partially raise the window.
2. Install the window run channel weatherstrip (2) to the guide channel.
3. Install the inner mirror garnish (2) to the front door.
4. Install the water deflector (3) to the front door (4).
5. Install the front side door trim. Refer to Front Side Door Trim Panel Replacement .