For 1990-2009 cars

### Removal Procedure

1. Raise the windshield wiper arm away from the windshield until the arm locks upright.
2. Swivel the windshield wiper blade on the wiper arm. Position the blade in order to access the release tab on the back side of the blade.
3. Push the retaining tab (3) and slide the wiper blade (2) toward the vehicle.
4. Slide the blade down the wiper arm until the blade moves past the hook (1).
5. Swivel the wiper blade to a 90 degree angle on the wiper arm.
6. Slide the wiper blade up.
7. Remove the wiper blade from the wiper arm.

### Installation Procedure

1. Slide the windshield wiper blade over the wiper arm past the hook.
2. Guide the retaining tab (3) into the hook (1). Slide the blade up until the tab (3) engages.
3. Lower the windshield wiper arm until the blade contacts the windshield.