For 1990-2009 cars

#### Tools Required

• | J 37271 Countershaft Locknut Spanner Wrench

• | J 8614-01 Countershaft Driven Gear Holder

• | J 34826 Hub Nut Socket

1. Unstake the countershaft driven gear locknut.
2. Install the J 8614-01 onto the countershaft driven gear (1) to hold the countershaft driven gear stationary during removal of the countershaft lock nut.
3. Use the J 34826 with a J 8614-01 to remove the countershaft driven gear (1) locknut from the countershaft.
4. Unstake the front countershaft locknut (2).
5. Use a J 37271 with a J 8614-01 in order to remove the front countershaft locknut from the countershaft assembly (1).
6. Use the J 8614-01 in order to remove the countershaft driven gear (2) from the countershaft.
7. Remove the J 8614-01 from the countershaft driven gear.
8. Remove the countershaft driven gear thrust bearing (2) from the transaxle case (1).
9. Remove the countershaft assembly (1) from the underdrive clutch assembly (2).
10. Remove the underdrive sun gear (1) from the underdrive clutch drum (2).
11. Remove the underdrive sun gear inner thrust bearing (3) from the underdrive clutch drum (1).