For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster assembly. Refer to Instrument Cluster Replacement .
2. Remove the instrument cluster lens (2) from the cluster retainer (1) by releasing the eight locking tabs.

### Installation Procedure

1. Align the lens (2) onto the guide pins and install the lens to the cluster retainer (1). Make sure that the locking tabs are fully engaged.
2. Install the instrument cluster assembly. Refer to Instrument Cluster Replacement .