For 1990-2009 cars

### Removal Procedure

1. Remove the front seat cushion. Refer to Front Seat Cushion Replacement .
2. Cut the hog rings (3).
3. Open the tabs.
4. Remove the seat cushion cover (1) from the seat cushion pad (2).
5. Remove the seat cushion pad (2) from the seat cushion frame (3).

### Installation Procedure

1. Install the seat cushion pad (2) to the seat cushion frame (3).
2. Install the seat cushion cover (1) to the seat cushion pad (2).
3. Secure the seat cushion cover (1) with new hog rings (3).
4. Install the front seat cushion. Refer to Front Seat Cushion Replacement .