For 1990-2009 cars

When the following conditions exist, inspect the rear compartment lid to the quarter panel gap for the proper alignment:

• | The rear compartment lid is closed.

• | The rear compartment lid lock is engaged.

Adjust the lid from the original position. Perform the adjustments using the elongated holes in the rear compartment lid hinge.

Prior to performing any rear compartment lid lock or striker adjustments, properly align the rear compartment lid to the rear compartment opening using the hinge adjustment.

Perform the following steps in order to adjust the rear compartment lid:

1. Open the rear compartment lid.
2. Loosen the 4 rear compartment lid (1) mounting bolts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Adjust the rear compartment lid to quarter panel clearance gap to between 2.5-5.5 mm (0.10-0.22 in) on each side of the rear compartment lid.

Tighten
Tighten the rear compartment lid bolts to 7 N·m (62 lb in).

4. Lower the rear compartment lid.