For 1990-2009 cars

### Removal Procedure

1. Remove the front seat cushion. Refer to Front Seat Cushion Replacement .
2. Cut the hog rings.
3. Remove the following components from the seat cushion:

• | The hog rings (3)

• | The seat cushion cover (1)

4. Remove the seat cushion pad from the frame, if necessary.

### Installation Procedure

1. Install the seat cushion pad to the frame, if removed.
2. Install the seat cushion cover (1) to the seat cushion. Secure the cover with new hog rings (3).
3. Install the front seat cushion. Refer to Front Seat Cushion Replacement .