For 1990-2009 cars

### Removal Procedure

1. Remove the I/P assembly. Refer to Instrument Panel Assembly Replacement .
2. Remove the following components from the I/P:

• | The three screws

• | The defroster outlet duct

### Installation Procedure

1. Install the defroster outlet duct to the IP. Secure the outlet duct with the three screws.
2. Install the I/P assembly. Refer to Instrument Panel Assembly Replacement .