For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster retainer. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .

Important: Do not remove the needle from the engine tachometer. There is not a detent or flat spot on the shaft in order to indicate the correct placement.

2. Remove the 6 screws (3) which secure the engine tachometer to the instrument cluster case.
3. Remove the tachometer (1) from the instrument cluster case.

### Installation Procedure

1. Install the engine tachometer (1) to the instrument cluster case.
2. Secure the tachometer with the 6 screws (3).
3. Install the instrument cluster retainer. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .