For 1990-2009 cars

1. Measure the 1st-reverse brake assembly clearance (1) using a feeler gage (2).

• | The 1st-reverse brake assembly clearance should fall within 1.060-2.380 mm (0.0417-0.0937 in).

• | If the 1st-reverse brake assembly clearance is below 1.060 mm (0.0417 in), inspect the 1st-reverse brake assembly components for excessive wear or damage.

2. Remove the 1st-reverse brake snap ring (1) from the transaxle case.
3. Remove the following components from the transaxle case:

• | 1st-reverse brake flange

• | Six plates

• | Six discs