For 1990-2009 cars

## Air Outlet Replacement Left

### Removal Procedure

1. Remove the I/P drivers knee bolster reinforcement. Refer to Knee Bolster Replacement .
2. Remove the following components from the I/P assembly:

• | The plastic retainer (1)

• | The left I/P outer air outlet duct (2)

3. Remove the screw and the left I/P outer air outlet (1) from the I/P assembly.

### Installation Procedure

1. Install the left I/P outer air outlet (1) to the I/P. Secure the outlet with the screw.
2. Install the left I/P outer air outlet duct (2) to the I/P. Secure the outlet duct with the plastic retainer (1).
3. Install the I/P drivers knee bolster reinforcement. Refer to Knee Bolster Replacement .

## Air Outlet Replacement Center

### Removal Procedure

1. Remove the I/P assembly. Refer to Instrument Panel Assembly Replacement .
2. Remove the following components from the I/P:

• | The one screw

• | The right I/P outer air outlet duct

• | The four screws

• | The I/P center air outlet

### Installation Procedure

1. Install the I/P center air outlet to the I/P. Secure the outlet duct with the four screws.
2. Install the right I/P outer air outlet duct to the I/P. Secure the outlet duct with the screw.
3. Install the I/P assembly. Refer to Instrument Panel Assembly Replacement .

## Air Outlet Replacement Right

### Removal Procedure

1. Remove the I/P assembly. Refer to Instrument Panel Assembly Replacement .
2. Remove the following components from the I/P:

• | The one screw

• | The right I/P outer air outlet duct

• | The two screws

• | The right I/P outer air outlet

### Installation Procedure

1. Install the right I/P outer air outlet to the I/P. Secure the outlet with the two screws.
2. Install the right I/P outer air outlet duct to the I/P. Secure the outlet duct with the screw.
3. Install the I/P assembly. Refer to Instrument Panel Assembly Replacement .