For 1990-2009 cars

#### Tools Required

• | J 8092 Universal Driver

• | J 25070 Heat Gun - 500-750 F

• | J 44741 Shift Rail Bearing Installer

• | J 44745 Countershaft Bearing Race Installer

• | J 44746 Mainshaft/Input Shaft Bearing Race Installer

1. Using the J 25070 , heat the intermediate case for 10-15 minutes.
2. Install the countershaft bearing race in the intermediate case using the J 8092 (1) and the J 44745 (2).
3. Install the mainshaft intermediate bearing race in the intermediate case using the J 8092 (1) and the J 44746 (2).
4. Install the shift rail bearing in the intermediate case using the J 8092 (1) and the J 44741 (2).