For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat back cushion. Refer to Rear Split Folding Seat Back Replacement .
2. Remove the following components from the vehicle:

• | The 2 bolts which secure the rear seat back cushion outer pivot support

• | The rear seat back cushion outer pivot support (1)

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the rear seat back cushion outer pivot support (1) to the vehicle. Secure the support with the 2 bolts.

Tighten
Tighten the outer pivot support bolts to 7.9 N·m (70 lb in).

2. Install the rear seat back cushion. Refer to Rear Split Folding Seat Back Replacement .