For 1990-2009 cars

(1) | Front Suspension Strut Bolt
(2) | Steering Knuckle
(3) | Front Lower Control Arm Ball Stud
(4) | Front Lower Control Arm Ball Stud Nut
(5) | Steering Knuckle Cotter Pin
(6) | Front Suspension Strut Nut

The front steering knuckle is made of steel. Do not use a hammer to loosen suspension components from the steering knuckle. Suspension components attached to the steering knuckle (i.e. ball joint/stud, strut damper) are made of steel and have special coatings to prevent corrosion.