For 1990-2009 cars

1. Remove following components:

• | The crankshaft position sensor bolt (5)

• | The sensor

2. Remove the drive belt tensioner nut.
3. Remove the following components from the mounting surface.

• | The drive belt tensioner bolt

• | The tensioner

4. Remove the following fasteners:

• | The timing chain cover bolts (2-14)

• | The nuts (1 & 5)

5. Gently pry the timing chain cover away from the cylinder block and remove the timing chain cover.