For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Cable Adjusting Locknuts | 8 N·m | 71 lb in
Accelerator Cable Attaching Screws | 2 N·m | 26 lb in
Accelerator Cable-to-bulkhead Bolts | 15 N·m | 11 lb ft
Accelerator Pedal Cable-to-bulkhead Bolts | 15 N·m | 11 lb ft
Air Cleaner Lower Assembly Bolts | 15 N·m | 11 lb ft
Accelerator Pedal Bracket Bolts | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 8.8 N·m | 77 lb in
Camshaft Position (CMP) Sensor Bolt | 8.8 N·m | 77 lb in
Engine Coolant Temperature (ECT) Sensor | 20 N·m | 14 lb ft
EVAP Canister Support Bracket Bolts | 18.5 N·m | 13 lb ft
EVAP Canister Purge Solenoid Valve Bolt | 15 N·m | 11 lb ft
Fuel Injector Wiring Harness Bolts | 8.8 N·m | 77 lb in
Fuel Injector Wire Harness Cover Plate Bolt | 8.8 N·m | 77 lb in
Fuel Injector Wire Harness Cover Plate Nuts | 8 N·m | 71 lb in
Fuel Rail Bolts | 18.5 N·m | 13 lb ft
Fuel Rail Inlet Pipe Hold Nut | 8 N·m | 71 lb in
Fuel Sender Assembly Hold Down Plate Bolts | 4 N·m | 35 lb in
Fuel Tank Retaining Strap Bolts | 39 N·m | 29 lb ft
Heated Oxygen Sensor (HO2S) 1 | 44 N·m | 32 lb ft
Heated Oxygen Sensor (HO2S) 2 | 44 N·m | 32 lb ft
Ignition Coil Bolts | 8.8 N·m | 77 lb in
Intake Manifold Bolts | 18.5 N·m | 13 lb ft
Knock Sensor (KS) | 39 N·m | 29 lb ft
Negative Battery Cable Terminal Retainer Bolt | 15 N·m | 11 lb ft
PCM Mounting Bolts | 15 N·m | 11 lb ft
Power Steering Pressure (PSP) Switch | 21 N·m | 15 lb ft
Throttle Body/Accelerator Cable Bracket Bolt | 20 N·m | 15 lb ft
Throttle Body Nuts | 20 N·m | 15 lb ft
Vehicle Speed Sensor (VSS) Bolt | 9.3 N·m | 82 lb in