For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Radio/Audio System Check? | -- | Go to Step 2 | Go to Radio/Audio System Check
2 | Using a J 35616-200 backprobe the radio connector cavity 11 to ground. Does the test lamp light? | -- | Go to Step 3 | Go to Step 4
3 | Replace the radio. Refer to Radio Replacement . Is the replacement complete? | -- | Go to Radio/Audio System Check | --
4 | Repair the short in the BLU/YEL wire between the Junction Block 3, C 1 and the radio connector cavity 11. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Radio/Audio System Check | --