For 1990-2009 cars

# Labor Time Guide Updates - April 1999

Subject: | Warranty Administration -- April, 1999 Labor Time Guide Updates

Models: | 1994-2000 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

Important: Please retain any changes made to the A, B, D and L Car Labor Time Guides as these vehicles have been discontinued since 1997 and the Labor Time Guides will not be republished. Changes to the P/H Truck Chassis should also be retained. The vehicle was discontinued in December, 1998. Please note: Labor Time Guides for these discontinued vehicles will not be republished.

#### LTG Update - C/K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
DRIVER, FUEL PUMP SOLENOID (DIESEL) - REPLACE

- POLICY: D,E

R

J5974

2.4

2.4

2.4

2.4

2.4

2.4

2.4

ADD:

- A- With EGR L56 Engine (Code S)

N

0.2

0.2

0.2

0.2

0.2

0.2

0.2

- B- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

- C- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers If Nec

N

0.4

0.4

0.4

0.4

0.4

0.4

0.4

*IND: N - New/R - Revised

#### LTG Update -C/K Platform - New Body Style

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
WHEEL ALIGNMENT - CHECK AND/OR ADJUST

- No Change to "INC" or "NOTE"

No Change to "ADD" Conditions

R

E2020

--

--

--

--

--

0.8

0.8

*IND: N - New/R - Revised

#### LTG Update - F Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
FILLER, TAIL LAMP - REPLACE |  |  |  |  |  |  |  |  |
CENTER | N | B1093 | -- | -- | -- | 0.3 | 0.3 | 0.3 | 0.3
PRE-DELIVERY INSPECTION - BASE TIME | R | Z7000 |  |  |  |  |  |  |
CHEVROLET |  |  | -- | -- | 1.4 | 1.4 | 1.4 | 1.4 | 1.4
PONTIAC |  |  | -- | -- | 1.4 | 1.4 | 1.4 | 1.4 | 1.4
ADD: |  |  |  |  |  |  |  |  |

- A- To Install Sunshade Package

--

--

0.1

0.1

0.1

0.1

0.1

- B- To Install R/S Package (Chevrolet Only)

--

--

0.2

0.2

--

--

--

*IND: N - New/R - Revised

#### LTG Update - G Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
HOSES, HEATER (WITH AIR CONDITIONING) - REPLACE PART GP: 8.846 |  |  |  |  |  |  |  |  |
INLET |  | D2774 | -- | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
OUTLET |  | D2775 |  |  |  |  |  |  |
ENGINE CODE K |  |  | -- | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
ENGINE CODE 1 |  |  | -- | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
INLET AND OUTLET | N | D2779 |  |  |  |  |  |  |
ENGINE CODE C |  |  | -- | -- | -- | 1.4 | 1.4 | 1.4 | 1.4
WATER PUMP TO CORE |  | D2780 |  |  |  |  |  |  |
ENGINE CODE C |  |  | - | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
WATER VALVE TO CORE |  | D2781 |  |  |  |  |  |  |
ENGINE CODE C |  |  | -- | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
MANIFOLD TO CORE |  | D2782 |  |  |  |  |  |  |
ENGINE CODE C |  |  | -- | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
ALL HOSES |  | D2787 | -- | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6
*IND: N - New/R - Revised

#### LTG Update - G VAN Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96-F | 96-1 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | T | V | W | X | Y
MODULE, GLOW PLUG CONTROL (DIESEL) - REPLACE POLICY: D | N |  |  |  |  |  |  |  |  |
CONTROLLER/RELAY |  | J4820 | 0.5 | 0.5 | 0.5 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7
No Change to "ADD" Condition
*IND: N - New/R - Revised

#### LTG Update - J Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
REFLECTOR, REAR BUMPER - R&R OR REPLACE PART GP: 7.831 |  |  |  |  |  |  |  |  |
RIGHT | R | B0740 | 1.1 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
LEFT | R | B0741 | 1.1 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
*IND: N - New/R - Revised

#### LTG Update - J, L, N Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
93 | 94 | 95 | 96 | 97 | 98 | 99
YEAR VIN CODE
P | R | S | T | V | W | X
INSULATOR AND/OR BRACKET, FRONT STABILIZER SHAFT AT FRAME - REPLACE |  | E2180 | Refer to Bulletin 73-33-01A for applicable times

- PART GP: 7.243
- INC: one or both sides
- NOTE: Add time is for use only in conjunction with Service Bulletin 73-33-01A

ADD:

- A- To sand stabilizer shaft and apply tape to stabilizer bushing

N

J Platform |  |  | 0.2 | 0.2 | -- | -- | -- | -- | --
L Platform |  |  | 0.2 | 0.2 | 0.2 | 0.2 | -- | -- | --
N Platform |  |  | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | --
*IND: N - New/R - Revised

#### LTG Update - KD/KE Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
DRUM, BRAKE - R&R OR REPLACE

- PART GP: 5.809
- INC: Clean, inspect and adjust brakes.

REAR |  |  |  |  |  |  |  |  |
RIGHT |  | H0200 | -- | -- | -- | 0.4 | 0.4 | 0.4 | 0.4
LEFT |  | H0201 | -- | -- | -- | 0.4 | 0.4 | 0.4 | 0.4
BOTH |  | H0207 | -- | -- | -- | 0.5 | 0.5 | 0.5 | 0.5
ADD:

- A- To Reface Drum

- One

--

--

--

0.4

0.4

0.4

0.4

- Both

N

--

--

--

0.7

0.7

0.7

0.7

*IND: N - New/R - Revised

#### LTG Update - KS/KY Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
ADJUSTER ASSEMBLY, FRONT SEAT POWER - R&R OR REPLACE PART GP: 11.561 |  |  |  |  |  |  |  |  |
BUCKET SEAT |  |  |  |  |  |  |  |  |
PASSENGER | R | C6040 | 0.6 | 0.6 | 0.6 | 0.6 | 1.9 | 1.9 | 1.9
DRIVER | R | C6041 | 0.6 | 0.6 | 0.6 | 0.6 | 1.9 | 1.9 | 1.9
*IND: N - New/R - Revised

#### LTG Update - M/L Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
MODULE, TRANSFER CASE SHIFT - REPLACE | N | K4122 | -- | -- | -- | -- | -- | 0.7 | 0.7
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

--

--

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - N Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
MOTOR AND/OR FAN, BLOWER - R&R OR REPLACE

- PART GP: 9.215

HEATER (NON A/C) |  | D1320 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
A/C | R | D1322 |  |  |  |  |  |  |
4 CYL |  |  | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
6 CYL |  |  | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.3 | 0.3
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

BEARING AND HUB ASSEMBLY, FRONT WHEEL - REPLACE |  |  |  |  |  |  |  |  |
RIGHT |  | E2320 |  |  |  |  |  |  |
MALIBU & CUTLASS | R |  | -- | -- | -- | 0.8 | 0.8 | 0.8 | 0.8
ACHIEVA & SKYLARK |  |  | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | -- | --
GRAND AM & ALERO | R |  | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.8 | 0.8
LEFT |  | E2321 |  |  |  |  |  |  |
MALIBU & CUTLASS | R |  | -- | -- | -- | 0.8 | 0.8 | 0.8 | 0.8
ACHIEVA & SKYLARK |  |  | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | -- | --
GRAND AM & ALERO | R |  | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.8 | 0.8
BOTH |  | E2327 |  |  |  |  |  |  |
MALIBU & CUTLASS | R |  | -- | -- | -- | 1.0 | 1.0 | 1.0 | 1.0
ACHIEVA & SKYLARK |  |  | 1.2 | 1.2 | 1.2 | 1.2 | 1.2 | -- | --
GRAND AM & ALERO | R |  | 1.2 | 1.2 | 1.2 | 1.2 | 1.2 | 1.0 | 1.0
No Change to "ADD" Conditions
*IND: N - New/R - Revised

#### LTG Update - S Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
COIL, ELECTRONIC IGNITION CONTROL (DIS/3CI) - REPLACE | N | J4345 | -- | -- | -- | -- | 0.2 | 0.2 | 0.2
ADD: |  |  |  |  |  |  |  |  |

- A- To Replace Each Additional Coil

--

--

--

--

0.2

0.2

0.2

- B- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

--

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - S/T Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
CORE, HEATER - REPLACE

- PART GP: 8.854
- INC: Disable and Enable SIR System

HEATER (NON A/C) |  | D2820 | 2.2 | 2.3 | 2.3 | 2.3 | 3.3 | 3.3 | 3.3
A/C | R | D2822 |  |  |  |  |  |  |
LEFT HAND DRIVE |  |  |  |  |  |  |  |  |
UTILITY |  |  | 2.2 | 4.1 | 4.1 | 5.8 | 5.8 | 5.8 | 5.8
PICK-UP |  |  | 2.2 | 4.0 | 4.0 | 5.8 | 5.8 | 5.8 | 5.8
RIGHT HAND DRIVE |  |  | -- | -- | -- | -- | -- | 5.4 | 5.4
ADD:

- A- W/Radio

0.1

0.1

0.1

0.1

0.1

0.1

0.1

MANIFOLD AND/OR GASKET, INTAKE LOWER - R&R OR REPLACE

- No Change to "POLICY" or "NOTE"
- NOTE: Applies to Engine Code W, Z, X

R

J0224

2.4

2.4

2.5

2.5

2.5

2.5

2.5

ADD: A- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers If Nec |  |  | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
B- With A/C |  |  | -- | -- | 0.2 | 0.2 | 0.2 | 0.2 | 0,2
*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
REGULATOR, FRONT DOOR WINDOW - R&R OR REPLACE

- PART GP: 10.783
- No Change to "INCs" or "NOTE"

RIGHT MANUAL |  | C0180 | 0.8 | 0.8 | 0.8 | 0.8 | -- | -- | --
LEFT MANUAL |  | C0181 | 0.8 | 0.8 | 0.8 | 0.8 | -- | -- | --
RIGHT POWER |  | C0182 |  |  |  |  |  |  |
CHEVROLET |  |  | 0.8 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0
PONTIAC |  |  | 1.1 | 1.1 | 1.1 | 0.7 | 0.7 | 0.7 | 0.7
OLDSMOBILE |  |  | 1.1 | 1.1 | 1.1 | 1.1 | 0.7 | 0.7 | 0.7
BUICK |  |  | 1.1 | 1.1 | 1.1 | 0.7 | 0.7 | 0.7 | 0.7
LEFT POWER |  | C0183 |  |  |  |  |  |  |
CHEVROLET |  |  | 0.8 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0
PONTIAC |  |  | 1.1 | 1.1 | 1.1 | 0.7 | 0.7 | 0.7 | 0.7
OLDSMOBILE |  |  | 1.1 | 1.1 | 1.1 | 1.1 | 0.7 | 0.7 | 0.7
BUICK |  |  | 1.1 | 1.1 | 1.1 | 0.7 | 0.7 | 0.7 | 0.7
ADD: A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis | R |  | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3
MODULE, ELECTRONIC IGNITION CONTROL (DIS/3CI) - REPLACE No Change to "PART GP" or "POLICY" |  | J4343 |  |  |  |  |  |  |
ENGINE CODE X |  |  | 1.8 | 1.8 | 0.5 | 0.5 | -- | -- | --
ENGINE CODE M |  |  |  |  |  |  |  |  |
EXC CHEVROLET | R |  | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
CHEVROLET |  |  | 0.3 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6
ENGINE CODE T |  |  | 2.0 | -- | -- | -- | -- | -- | --
ENGINE CODE L AND 1 |  |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
ENGINE CODE K |  |  | 0.5 | 0.5 | 0.5 | 0.4 | 0.4 | 0.4 | 0.4
No Change to "ADD" Condition |  |  |  |  |  |  |  |  |
RESISTER, FUEL PUMP - REPLACE | R | J5612 |  |  |  |  |  |  |
WITHOUT WASHER BOTTLE |  |  | -- | -- | 0.3 | 0.3 | -- | -- | --
WITH WASHER BOTTLE |  |  | -- | -- | -- | -- | 1.3 | 1.3 | 1.3
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - Y Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
FRAME, SEAT BACK FRONT - REPLACE |  |  |  |  |  |  |  |  |
PASSENGER | N | C6835 |  |  |  |  |  |  |
SPORT SEAT |  |  | -- | -- | -- | 0.8 | 0.8 | 0.8 | 0.8
BASE SEAT |  |  | -- | -- | -- | 0.7 | 0.7 | 0.7 | 0.7
DRIVER | N | C6836 |  |  |  |  |  |  |
SPORT SEAT |  |  | -- | -- | -- | 0.8 | 0.8 | 0.8 | 0.8
BASE SEAT |  |  | -- | -- | -- | 0.7 | 0.7 | 0.7 | 0.7
COVER AND/OR PAD, FRONT SEAT INSERT PILLOW - REPLACE |
PASSENGER | N | C6995 |  |  |  |  |  |  |
SPORT SEAT |  |  | -- | -- | -- | 0.8 | 0.8 | 0.8 | 0.8
DRIVER | N | C6996 |  |  |  |  |  |  |
SPORT SEAT |  |  | -- | -- | -- | 0.8 | 0.8 | 0.8 | 0.8
COVER AND/OR PAD, FRONT SEAT BACK CUSHION - R&R OR REPLACE

- PART GP: 14.800
- POLICY: S Additional .3 hours if the vehicle is delivered to and from the repair location.
- NOTE: Applies to inner or outer cushion

BUCKET SEAT |  |  |  |  |  |  |  |  |
PASSENGER | R | C7050 |  |  |  |  |  |  |
SPORT SEAT |  |  | 0.7 | 0.7 | 0.7 | 0.4 | 0.4 | 0.4 | 0.4
BASE SEAT |  |  | 0.7 | 0.7 | 0.7 | 0.3 | 0.3 | 0.3 | 0.3
DRIVER | R | C7051 |  |  |  |  |  |  |
SPORT SEAT |  |  | 0.7 | 0.7 | 0.7 | 0.4 | 0.4 | 0.4 | 0.4
BASE SEAT |  |  | 0.7 | 0.7 | 0.7 | 0.3 | 0.3 | 0.3 | 0.3
No Change to "ADD" Conditions |  |  |  |  |  |  |  |  |
*IND: N - New/R - Revised