For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (IP) compartment. Refer to Instrument Panel Compartment Replacement .
2. Disconnect the blower motor electrical connector.
3. Remove the 3 screws and the blower motor and fan (1) from the vehicle.

### Installation Procedure

1. Install the blower motor and fan (1) to the vehicle. Secure with the 3 screws.
2. Connect the blower motor electrical connector.
3. Install the IP compartment. Refer to Instrument Panel Compartment Replacement .