For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: Both Low Beams Inoperative
1 | Were you sent here from the Headlamp System Check? | -- | Go to Step 2 | Go to Headlight System Check
2 |

1. Remove the DIMMER relay.
2. Connect a fused jumper wire from cavity 1 to cavity 4 of the socket where the DIMMER relay came from.
3. Turn the light switch to the head position.

Do the low beams illuminate?

--

Go to Step 3

Go to Step 4

3 | Replace the DIMMER relay. Is the replacement complete? | -- | Go to Headlight System Check | --
4 | Locate and repair the open in the BLK wires between the DIMMER relay and the fuses. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Headlight System Check | --