For 1990-2009 cars

### Removal Procedure

1. Remove the rear door jamb switch mounting screw from the door jamb.
2. Disconnect the rear door jamb switch electrical connector.
3. Remove the door jamb switch (2) from the vehicle.

### Installation Procedure

1. Connect the rear door jamb switch electrical connector.
2. Install the rear door jamb switch (2) to the door jamb. Secure the door jamb switch with the screw.