For 1990-2009 cars

Problem | Action
--- | ---
Low or no fluid | Add fluid.
Shift cable out of adjustment, binding or damaged | Adjust or replace the select cable.
Parking lock pawl mechanism locked or frozen | Inspect the parking lock pawl.
Broken torque converter to flywheel bolts | Replace the bolts.
Torque converter stator one-way clutch no holding | Replace the torque converter.
Torque converter failure | Replace the torque converter.
Valve body spacer plate or gaskets improper position or damaged | Inspect the valve body.
The check balls are omitted or improper position | Inspect the valve body.
Manual valve binding or sticking | Inspect the valve body.
Manual valve link disconnected | Inspect the manual valve linkage.
Incorrect line pressure | Perform the line pressure diagnosis.