For 1990-2009 cars

### Removal Procedure

1. Remove the following along the top of the front bumper fascia:

• | The 2 bolts (1)

• | The plastic retainer (2)

2. Raise and suitably support the vehicle at a desired height. Refer to Lifting and Jacking the Vehicle in General Information.
3. Loosen the front wheelhouse panel liners (1) on both sides of the vehicle in order to gain access to the front bumper fascia to fender bolts and the front bumper fascia brace upper bolts.
4. Remove the front bumper fascia to fender bolt (1) from each side of the fascia (2).
5. Remove the front bumper fascia brace upper bolt (1) from each side of the fascia (2).
6. Remove the 2 plastic retainers from the bottom of the front bumper fascia.
7. Pull the front bumper fascia (2) forward and remove the fascia from the vehicle.
8. Remove the following components from the front bumper fascia:

• | The 2 plastic retainers (2)

• | The front bumper fascia braces (1)

### Installation Procedure

1. Install the front bumper fascia braces (1) to the fascia. Secure each brace with 1 plastic retainer (2).
2. Install the front bumper fascia (2) to the vehicle.
3. Install the 2 plastic retainers to the bottom of the front bumper fascia.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the front bumper fascia brace upper bolt (1) to each side of the front bumper fascia (2).

Tighten
Tighten the front bumper fascia brace upper bolts to 5 N·m (43 lb in).

5. Install the front bumper fascia to fender bolt (1) to each side of the fascia (2).

Tighten
Tighten the front bumper fascia to fender bolts to 2 N·m (18 lb in).

6. Reposition and secure the front wheelhouse panel liners (1).
7. Lower the vehicle.
8. Install the 2 bolts (1) and the plastic retainer (2) along the top of the front bumper fascia.

Tighten
Tighten the upper front fascia bolts to 5 N·m (43 lb in).