For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the front bumper fascia energy absorber (1) from the front bumper impact bar.

### Installation Procedure

1. Install the front bumper fascia energy absorber (1) to the front bumper impact bar.
2. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .