For 1990-2009 cars

### Removal Procedure

1. Remove the drum. Refer to Brake Drum Replacement .
2. Remove the brake shoes (6,14) and the hardware (1,2,3,4,5,7,8,9,10,11,12,13,15,16,17,18). Refer to Brake Shoe Replacement .

### Installation Procedure

Important: Apply Lubriplate® GM P/N 1050109 white lithium grease, or the equivalent, to all of the brake component metal contact points (where the brake shoe metal contacts the backing plate, the wheel cylinder and the adjustment strut, etc.) prior to installation.

1. Install the drum brake hardware components (1,2,3,4,5,7,8,9,10,11,12,13,15,16,17,18).
2. Install the brake shoes (6,14). Refer to Brake Shoe Replacement .
3. Install the drum. Refer to Brake Drum Replacement .