For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the following components from the vehicle:

• | The 6 bolts

• | The engine splash shield (1)

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the engine splash shield (1) to the vehicle. Secure the splash shield with the 6 bolts.

Tighten
Tighten the engine splash shield bolts to 10 N·m (89 lb in).

2. Lower the vehicle.