For 1990-2009 cars

### Removal Procedure

1. Gently pry loose the high mounted stoplamp and cover assembly (2).
2. Disconnect the high mounted stoplamp electrical connector.
3. Remove the assembly from the vehicle.
4. Unclip the 6 plastic retainers (1) from each and remove the quarter upper trim panels (2).
5. Push in the tab (3) on the headrest guide.
6. Remove each of the head restraints (1) from the vehicle.
7. Remove the following components from the vehicle:

• | The 2 plastic retainers (1)

• | The rear window trim panel (2).

### Installation Procedure

1. Install the rear window trim panel (2). Secure the trim panel with the 2 plastic retainers (1).
2. Align the head restraint posts into the head rest guides.
3. Push in the tab (3) on the head restraint guide in order to install each of the head restraints (1) to the vehicle. Ensure that the retainer lock engages.
4. Install the quarter upper trim panels (2). Ensure that the plastic retainers are fully engaged.
5. Connect the high mounted stoplamp electrical connector.
6. Install the high mounted stoplamp and cover assembly (2) to the vehicle.