For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Were you sent here from the Interior Light Dimming System Check? | -- | Go to Step 2 | Go to Interior Lights Dimming System Check
2 | Inspect the WHT/GRN wire between the IP lamp controller cavity 3 and junction block 3, C3 cavity 17 for an open or bad connections. Did you find any opens or bad connections? | -- | Go to Step 3 | Go to Step 5
3 | Repair any opens and/or any bad connections in the WHT/GRN wire. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Interior Lights Dimming System Check | --
4 | Replace the IP lamp controller. Refer to Instrument Panel Lamp Dimmer Switch Replacement in Instrument Panel, Gauges, and Console. Is the replacement complete? | -- | Go to Interior Lights Dimming System Check | --
5 | Inspect the GRN wire between the IP lamp controller cavity 1 and junction block 3, C4 cavity 7 for an open or bad connections. Did you find any open or bad connections? | -- | Go to Step 6 | Go to Step 4
6 | Repair the open and or any bad connections in the GRN wire. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Interior Lights Dimming System Check | --