For 1990-2009 cars

#### RH Mirror Inoperative

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: The LH mirror does not move UP or DOWN, LEFT or RIGHT.
1 | Were you sent here from the Outside Mirror System Check? | -- | Go to Step 2 | Go to Outside Mirrors System Check
2 | Can the power mirror move in any direction? | -- | Go to Step 3 | Go to Step 12
3 | Can the power mirror move left and right? | -- | Go to Step 4 | Go to Step 9
4 |

1. Disconnect the RH front outside rearview mirror assembly connector.
2. Using a test lamp, front probe cavity 3 to ground.

When you activate the RH switch to the UP position does the test lamp illuminate?

--

Go to Step 5

Go to Step 6

5 | Replace the RH front power mirror assembly. Refer to Power Mirror Replacement . Is the replacement complete? | -- | Go to Outside Mirrors System Check | --
6 | Test the RED/GRN wire between the outside rearview mirror switch and the mirror assembly for an open. Does the wire have an open in it? | -- | Go to Step 8 | Go to Step 7
7 | Replace the power mirror switch. Refer to Power Mirror Switch Replacement . Is the replacement complete? | -- | Go to Outside Mirrors System Check | --
8 | Repair the open in the RED/GRN wire between the outside rearview mirror switch and the mirror assembly. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
9 |

1. Disconnect the RH front outside rearview mirror assembly connector.
2. Using a test lamp, front probe cavity 1 to ground.

When you activate the switch to the LEFT position does the test lamp illuminate?

--

Go to Step 5

Go to Step 10

10 | Test the RED wire between the switch and the mirror assembly for an open? Does the wire have an open in it? | -- | Go to Step 7 | Go to Step 11
11 | Repair the open in the RED wire. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
12 |

1. Disconnect the RH front outside rearview mirror assembly connector.
2. Using a test lamp, front probe cavity 2 to ground.

When you activate the switch to the DOWN position does the test lamp illuminate?

--

Go to Step 5

Go to Step 13

13 | Test the BRN/RED wire between the outside rearview mirror switch and the mirror assembly for an open in it. Does the wire have an open in it? | -- | Go to Step 7 | Go to Step 14
14 | Repair the open in the BRN/RED wire. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --