For 1990-2009 cars

## Compressor Shaft Seal Removal V5 - Direct Mount

#### Tools Required

• | J 41790-A Compressor Holding Tool

• | J 42136 A/C Lip Seal Remover

1. Place the compressor on the J 41790-A .
2. Remove the compressor clutch plate and hub assembly. Refer to Compressor Clutch Plate and Hub Assembly Removal (V5 - Direct Mount) .
3. Remove the compressor shaft seal retainer ring (2), using internal snap ring pliers (1).
4. To keep any dirt or foreign material from getting into the compressor, thoroughly clean the following components:

• | The inside of the compressor neck area surrounding the shaft

• | The exposed portion of the compressor shaft seal

• | The compressor shaft

• | The O-ring groove

5. Fully engage the lip of the J 42136 into the recessed portion of the seal (1) then turn the handle clockwise.
6. Remove the compressor shaft seal from the compressor with a rotary pulling motion.
7. Recheck the shaft and inside of the compressor neck for dirt or foreign material and make sure these areas are perfectly clean before installing the new compressor shaft seal.