For 1990-2009 cars

### Removal Procedure

1. Remove the center console trim bezel. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gauges and Console.
2. Remove the two screws (5) and pull the heater control unit (4) forward.
3. Remove the illumination bulbs (2).

### Installation Procedure

1. Install the illumination bulbs (2).
2. Install the heater control unit (4) to the instrument panel (IP). Secure with the two screws (5).
3. Install the center console trim bezel. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gauges and Console.