For 1990-2009 cars

### Removal Procedure

Remove the following components from the vehicle:

• | The trim covers (2)

• | The 2 screws

• | The rear assist handle (1) with a coat hook

### Installation Procedure

1. Install the rear assist handle (1) and coat hook assembly to the roof. Secure the handle assembly with the 2 screws.
2. Install the rear assist handle trim covers (2) that conceal the screws.