For 1990-2009 cars

### Removal Procedure

1. Remove the center console trim bezel. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gages and Console.
2. Remove the 2 screws and pull the HVAC control unit forward.
3. Remove the 2 screws and the fresh/recirc switch.
4. Disconnect the blower speed selector switch electrical connector.
5. Disconnect the A/C switch electrical connector.
6. Remove the following from the HVAC control unit:

• | The temperature control cable

• | The mode control cable

7. Remove the HVAC control unit.

### Installation Procedure

1. Install the following to the HVAC control unit:

• | The temperature control cable

• | The mode control cable

2. Connect the blower speed selector switch electrical connector.
3. Connect the A/C switch electrical connector.
4. Install the fresh/recirc switch. Secure with the 2 screws.
5. Install the HVAC control unit to the instrument panel. Secure with the 2 screws.
6. Install the center console trim bezel. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gages and Console.
7. Adjust the cables as necessary, refer to the following:

• | Temperature Control Cable Adjustment

• | Mode Control Cable Adjustment