For 1990-2009 cars

### Removal Procedure

1. Remove the rear window trim panel. Refer to Rear Window Trim Panel Replacement in Body Rear End.
2. Disconnect the rear speaker electrical connector.
3. Remove the rear speaker mounting bolt (3).
4. Remove the rear speaker (2) from the vehicle.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the rear speaker (2) to the vehicle. Secure the speaker with 1 bolt (3).

Tighten
Tighten the speaker bolt to 10 N·m (89 lb in).

2. Connect the rear speaker electrical connector.
3. Install the rear window trim panel. Refer to Rear Window Trim Panel Replacement in Body Rear End.