For 1990-2009 cars

### Removal Procedure

1. Remove the 2 fasteners from the engine cover.
2. Remove the 2 plastic retainers from the engine cover.
3. Remove the engine cover (1) from the engine.
4. Remove the oil filter plug (4) of the camshaft position (CMP) actuator solenoid from the cylinder head (3).
5. Remove the oil filter (2) from the oil filter plug.

### Installation Procedure

1. Install the oil filter (2) into the oil filter plug of the CMP actuator solenoid.
2. Install the oil filter plug (4) with a new O-ring (1) into the cylinder head (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Tighten the oil filter plug.

Tighten
Tighten the plug to 21 N·m (15 lb ft).

4. Install the engine cover (1).
5. Secure the engine cover (1) with the 2 fasteners.

Tighten
Tighten the 2 fasteners to 8.8 N·m (77 lb in).

6. Install the 2 plastic retainers.