For 1990-2009 cars

## Radio Rear Speaker Replacement 2 Door

### Removal Procedure

1. Remove the rear quarter lower trim panel. Refer to Rear Quarter Lower Trim Panel Replacement in Interior Trim.
2. Remove the 3 screws (3) which secure the rear speaker (4) to the body.
3. Disconnect the rear speaker electrical connector (2).
4. Remove the rear speaker (1) from the vehicle.

### Installation Procedure

1. Connect the rear speaker electrical connector (2).
2. Install the rear speaker (4) to the vehicle. Secure the speaker with the 3 screws (3).
3. Install the rear quarter lower trim panel. Refer to Rear Quarter Lower Trim Panel Replacement in Interior Trim.

## Radio Rear Speaker Replacement 4 Door

### Removal Procedure

1. Remove the rear quarter lower trim panel. Refer to Rear Quarter Lower Trim Panel Replacement in Interior Trim.
2. Remove the 3 screws (2) which secure the rear speaker (1) to the body.
3. Disconnect the rear speaker electrical connector (1).
4. Remove the rear speaker (2) from the vehicle.

### Installation Procedure

1. Connect the rear speaker electrical connector (1).
2. Install the rear speaker (1) to the vehicle. Secure the speaker with the 3 screws (2).
3. Install the rear quarter lower trim panel. Refer to Rear Quarter Lower Trim Panel Replacement in Interior Trim.