For 1990-2009 cars

### Removal Procedure

1. Remove the parking brake lever bezel attaching screws (2).
2. Remove the parking brake lever bezel (1).
3. Remove the center console attaching screws (2).
4. Remove the center console (1).
5. Disconnect the 4WD switch electrical connector (2).
6. Remove the 4WD switch (3) from the transfer case (1).

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the 4WD switch (1) to the transfer case (2).

Tighten
Tighten the 4WD switch to 30 N·m (22 lb ft).

2. Connect the 4WD switch electrical connector (2).
3. Install the center console (1).
4. Install the center console attaching screws (2).
5. Install the parking brake lever bezel (1).
6. Install the parking brake lever bezel attaching screws (2).
7. Perform Diagnostic System Check - ABS .