For 1990-2009 cars

### Removal Procedure

1. Turn the lock knob (1) counterclockwise, and remove from each side of the crossrail .
2. Lift up crossrail.
3. Slide off and remove the luggage carrier crossrails (1) from the luggage carrier side rails (2).

### Installation Procedure

1. Install the luggage carrier crossrails, each are labeled front and rear (1) to the luggage carrier side rails (2).
2. Turn the lock knob (1) clockwise on each side of the luggage carrier crossrail in order to tighten the crossrail, be sure to tighten firmly.