For 1990-2009 cars

1. Install the turbocharger boost sensor to the intake manifold.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the turbocharger boost sensor bracket bolt.

Tighten
Tighten the turbocharger boost sensor bracket bolt to 10 N·m (89 lb in).

3. Install the intake manifold tube gaskets.
4. Install the intake manifold tube.
5. Install the intake manifold tube bolts and nuts.

Tighten
Tighten the intake manifold tube bolts and nuts to 9 N·m (80 lb in).

6. Install the intake air heater with gasket.

Tighten
Tighten the intake air heater to 25 N·m (18 lb ft).