For 1990-2009 cars

Point | Location | Clearance Gap (mm) | Flushness (mm)
--- | --- | --- | ---
1 | Side Window Pillar-to-Windshield Pillar | 5.2 mm (0.20 in) | 0-1.5 mm (0.0-.05 in)
2 | Hood-to-Fender | 4.5-7.1 mm (0.17-0.28 in) | --
3 | Hood-to-Front End Panel | 4.2-7.0 mm (0.16-0.27 in) | 0.0-1.5 mm (0.0-0.05 in)
4 | Hood-to-Air Inlet Grille | 3.7 mm (0.14 in) | --
5 | Air Inlet Grille-to-Fender | 4.8 mm (0.18 in) | --